Author: mike

DLPS-15C
SURGE SUPPRESSOR
Drop Line
The easy to install DLPS-15C protects drop line electronics from surges, transients, spikes and lightning. The DLPS-15C, using solid state Sidactor technology, protects in both directions from the house and from the cable drop line.

SOLID STATE
SURGE SUPPRESSION

DOCSIS 3.1
5-1218 MHZ

SPECIFICATIONS
Power Passing	Up to 2 amps
Switching Voltage	135V Peak Min. 165V Peak Max.
Response Time	Less than 1 nanosecond
Current Suppression	500 Amps (2 x 10µs)

PERFORMANCE
Frequency	5-15 mhz	15-250 mhz	250-550 mhz	550-900 mhz	900-1000 mhz
Insertion loss	< 0.75dB	< 0.5dB	< 0.5dB	< 0.5dB	< 0.75dB
Return loss	> 21dB	> 21dB	> 21dB	> 21dB	> 21dB
EMI shielding	> 120dB	> 120dB	> 120dB	> 120dB	> 120dB

FEATURES
Attaches to ground block The DLPS-15C design allows for quick installation to the subscribers ground block.
Longer Life THE DLPS-15C performance will not degrade during repeated overvoltage conditions. A gas tube device’s performance rating is degraded each time an overvoltage occurs. You can count on the DLPS-15C on the 1st surge or the 5000th surge.
Sidactor® Device The DLPS-15C incorporates the newest solid state Sidactor technology which eliminates the need for gas tube type surge suppressors.
Overvoltages Taken off Center Conductor Patented design takes overvoltages directly to ground from the center conductor, before damage can occur to drop line electronics
High Current Handling DLPS-15C Handles 1000 Amps.	Two (2) Year Warranty
ISO 9001 The DLPS series is manufactured in an ISO 9001 facility	Meets NEC 830
Surge Testing ANSI C-62.41 (IEEE 587)

Specifications subject to change without notice.

.

4737 Hwy 332 Suite 21
Hoschton, GA 30548
770-969-5146
www.cableinnovations.com